NC-Hops needs its part origin front left. For machines with its origin left back for example Biesse machines we recommend to use "Stops Left (Biesse)" for the Partlayout. 
You will get an error message for any not allowed partorigin.
