# Release Notes interiorcad 2025 F3

### Fixes Sets

- Use the new searchable pulldown menu to disclose and find sets located in the vectorworks defaults folder, user folder or workgroup folder easily
- Navigate to the current user or workgroup folder right from within each set pulldown menu
- New searchable pulldown menu to access Cabinet 3D material sets in settings dialog and, for all sets, in Cabinet 3D's object info palette

### Fixes Drawers

- Custom suppliers were ignored für integrated sliders
- Occasionally, sets and fitting configurations couldn't be assigned
- Integrated wooden drawers / sliders can now be inset from the front of the Cabinet 3D

### Other Fixes

- Profiles can now be placed on custom parts with non-standard oriented pathsusing either interiorcad's profile tool or Vectorworks' symbol insertion tool
- Option "Interrupt grid drilling" is available if no grid drilling is assigned tothe Cabinet 3D object yet (e.g. for using a fitting configuration)
- Dado for back was too short for angled Cabinet 3D
- Horizontal / Vertical blind fronts have separate 2D/3D representation now
- Using integrated drawers sometimes added an additional slider right at thecabinet's insertion point
- Changing height of Cabinet 3D multiple times sometimes caused Vectorworks toquit unexpectedly
- Grid drillings on angled cabinets (viewed from the right) were not createdproperly after transforming the cabinet
- Continuous partitions dividing a slanted top board were not created properly
- Inset dados were not created properly for slanted parts of an angled cabinet

### Improvements / Fixes NC-Export / Cuttinglist-Export

- Custom Export

- The material properties -> Part (item number) -> supplier id and description were not transferred

- Cuttinglist-Export in general

- Box objects of different lengths are not cumulated

- Maestro Ottimo Cut - Incorrect conversion of the fixed date fixed
- NC-Export in general

- Clamex machine configurations and error messages improved
- The new Clamex fittings may have generated a TypeError when using {clamexcangle}.

### Improvements Libraries

- New System Drawers: Häfele Matrix Box P Plus as a set available in heights of 60 mm / 115 mm / 170 mm (custom heights in combination with Longside Rails)
- New Sliders for Wooden Drawers: Grass Dynaneo
- New Hinges and Mounting Plates: Grass MB object hinges
- FIX: Hettich ArciTech Drawer Boxes with Longside Rails

# Release Notes interiorcad 2025 F2 / F2.1

### Saved sets & fittings in workgroup folders

Saved sets & fittings can now be stored and maintained directly in a workgroup folder. No more need to navigate to the workgroup folder in the Finder / Explorer.

### Mix & match single and dual use hinges

interiorcad 2025 F2 allows the use of hinges for single use (door hinged to cabinet side) in a dual use context (door hinged to cabinet partition) and vice versa.

### Horizontal blind fronts

In addition to vertical blind fronts (fake door) interiorcad 2025 F2 now provides horizontally oriented blind fronts (fake drawer front).

### Fixes

- Continuous front / back stiles now split front / back stretcher correctly
- The descriptions of all parts of the Plinth 3D are correctly shortened by the file name filter of the exports
- Divisions of cabinet were always translated to absolute dimensions upon creation in the dialog (F2.1)

### Improvements / Fixes NC-Export / Cuttinglist-Export

- BiesseCIX / bSolid - In order to use the Lamello Clamex properly, it is necessary to override the original side generated by the NC macro and define a separate side in the NC macro code of the Clamex. To override the original side the strings "NAME=WFL" and "sideid" must be in the NC macro code. If this is the case, the side properties change their functionality.

### Improvements Libraries

- Lamello P-System 2024 with Drilling 3D and improved alignment for the following systems

- bSolid
- Zeta P2 handheld machine - drillings for positioning pins

- Hettich AvanTech YOU 2024 - series now with separate front fixings
- Hettich Frontstabilizer - new model

# Release Notes interiorcad 2025 F1

### Fixes

- Drillings and center punches of integrated mounting plates sometimes would not export properly
- AV list considers edge length addition
- 'Remove NC info' added to interiorcad workspaces
- Cabinet 3D - Deleting saved fitting configurations caused a crash

### Improvements / Fixes NC-Export / Cuttinglist-Export

- Custom Export

- Construction group of fittings was stile / shelf
- Search Filter for available fields
- The field thickness now outputs the overall thickness
- New field for thickness of backing material / covering
- Filter fittings by supplier(s)

- NC-Export in general

- NC Macro Code - new variable clamexcangleverticalplus180 for special cases of the Lamello Clamex, which adds 180 degrees to the clamexcangle when used on the vertical surface

- Maestro CNC - Tool configuration file (*.tlgx) was not found if only the name was entered instead of the full path
- Xilog Plus - "Parking position distance to workpiece" can now be empty

### Improvements Libraries

- Lamello P-System 2024 with Drilling 3D and improved alignment for the following systems

- F4Integrate
- Maestro CNC
- NC-Hops
- woodWOP
- Xilog Plus

- Egger - Top 60 textures from the scopes wood, plain and design
- FixChip nesting connectors for the following systems

- bSolid
- Maestro CNC

- Hinges "Inset Application" with indication of door overlay

### Upcoming service pack

interiorcad 2025 F4 scheduled for the week of March 31, 2025.

interiorcad 2025 F3 interiorcad 2025 F2 / F2.1 interiorcad 2025 F1 Upcoming service pack