# Release Notes interiorcad 2025 F4

### Performance Box Objects

Selecting, loading and creating Box Objects was sped up substantially. Please note: If you have created your own box objects in your user or workgroup folder, please open and re-save these files.

### Material Description / Comment (Preview)

The field "Description" of a Custom Part 3D's material is now mirrored in the Custom Part 3D's object info palette and can be edited there.

The value of the field "Description" of a Custom Part 3D's material now remains if a material set containing no description is loaded.

The value of the field "Comment" of a Custom Part 3D's material now remains if a material set containing no comment is loaded.

### Fixes

- External grid grillings were not migrated properly from previous versions (F4.2)
- Part-based external grid drillings were not exported correctly to Part Layout or NC-Export (F4.2)
- Top/Bottom distance of external grid drilling was mixed up if placed on a Cabinet 3D's right side (F4.2)
- Grid drillings on partitions based on a fixed shelf were not exported correctly to Part Layout or NC-Export (F4.2)
- Choosing custom box objects sometimes terminated Vectorworks unexpectedly if the custom box objects were located in nested folders within the user folder (F4.2)
- Material sets were not always loaded from the workgroup folder (F4.1)
- Integrated grid drilling created a spare drilling if applied to multiple boxes with grid drilling turned off
- When saving a fitting configuration, interiorcad sometimes complained that the configuration is empty
- Fitting configuration sometimes were reported as being inconsistent
- Continuous partitions designed as mitered were not created properly if the angled part was defined as a top board
- Depending on the selection, fittings were exported inconsistently
- 2D view of Cabinet 3D did not include a laid-on back
- Symbols contained in Box Object sets were not saved in workgroup folders
- Loading a set for fixed shelves reset option to turn off grid drilling in the cox containing the fixed shelf
- Dialog to edit fitting configurations did not show source of fitting configuration file (user / workgroup folder)
- Applying a fitting configuration stored in a workgroup folder did not apply drawers
- Option to open user and workgroup folder were mixed up in Cabinet 3D "Construction" dialog pane
- Integrated grid drillings could not be based on grids stored in workgroup folder
- Overwriting an existing fitting configuration sometimes removed another configuration
- Front details text on Cabinet 3D front panels was not formatted and aligned properly
- Fixes for migrating workgroup folders from older versions
- Custom system drawers stored in workgroup folders did not show up in Drawer 3D tool's mode bar
- Fittings placed on an angled Cabinet 3D object were created outside the cabinet
- Integrated drawers configured with previous versions did not show up with the correct specification in the Cabinet 3D's settings dialog
- Drill-through / route-through drillings and contours were not created with the correct depth in integrated wooden drawers
- Partitions for angled cabinets (front view) were not created properly if the option "Automatic" was set for the creation of angled parts and the cabinet's side / board thickness were different

### Improvements / Fixes NC-Export / Cuttinglist-Export

- productionManager (HOMAG) as new Cuttinglist output format

- The export creates a ZIP file with a user-definable path and name
- The parts list configuration contains further options for customizing the output
- Technically the ZIP file contains

- an XML file with a hierarchical structure according to project item, cabinet and custom part, each with all associated production details
- the simultaneously or previously created NC programs stored in subfolders of the same hierarchy

- In productionManager, the ZIP file can be opened using the command "Import new job"

- NC-Export in general

- WorkpieceComments extended: SupplierID, Length, Width, Thickness, BoardThickness, Covering1Thickness, Covering2Thickness, SetName, HasCovering, HasSizing

### Improvements Libraries

- New: Häfele screws - Washer head screws for back panels
- Update: Häfele screws - Sales info updated
- Update: Custom Part 3D materials now with empty description
- Update: Lamello P-System Connectors for Maestro CNC Schreinertraum
- Fix: Hettich Sensys hinge for inset applications now has correct secondary drillings

# Release Notes interiorcad 2025 F3

### Fixes Sets

- Use the new searchable pulldown menu to disclose and find sets located in the vectorworks defaults folder, user folder or workgroup folder easily
- Navigate to the current user or workgroup folder right from within each set pulldown menu
- New searchable pulldown menu to access Cabinet 3D material sets in settings dialog and, for all sets, in Cabinet 3D's object info palette

### Fixes Drawers

- Custom suppliers were ignored für integrated sliders
- Occasionally, sets and fitting configurations couldn't be assigned
- Integrated wooden drawers / sliders can now be inset from the front of the Cabinet 3D

### Other Fixes

- Profiles can now be placed on custom parts with non-standard oriented pathsusing either interiorcad's profile tool or Vectorworks' symbol insertion tool
- Option "Interrupt grid drilling" is available if no grid drilling is assigned tothe Cabinet 3D object yet (e.g. for using a fitting configuration)
- Dado for back was too short for angled Cabinet 3D
- Horizontal / Vertical blind fronts have separate 2D/3D representation now
- Using integrated drawers sometimes added an additional slider right at thecabinet's insertion point
- Changing height of Cabinet 3D multiple times sometimes caused Vectorworks toquit unexpectedly
- Grid drillings on angled cabinets (viewed from the right) were not createdproperly after transforming the cabinet
- Continuous partitions dividing a slanted top board were not created properly
- Inset dados were not created properly for slanted parts of an angled cabinet

### Improvements / Fixes NC-Export / Cuttinglist-Export

- Custom Export

- The material properties -> Part (item number) -> supplier id and description were not transferred

- Cuttinglist-Export in general

- Box objects of different lengths are not cumulated

- Maestro Ottimo Cut - Incorrect conversion of the fixed date fixed
- NC-Export in general

- Clamex machine configurations and error messages improved
- The new Clamex fittings may have generated a TypeError when using {clamexcangle}.

### Improvements Libraries

- New Special Connectors: FESTOOL Domino corner and worktop connectors (plus extra FESTOOL grids)
- New System Drawers: Häfele Matrix Box P Plus as a set available in heights of 60 mm / 115 mm / 170 mm (custom heights in combination with Longside Rails)
- New Sliders for Wooden Drawers: Grass Dynaneo
- New Hinges and Mounting Plates: Grass MB object hinges
- Fix: Hettich ArciTech Drawer Boxes with Longside Rails

# Release Notes interiorcad 2025 F2 / F2.1

### Saved sets & fittings in workgroup folders

Saved sets & fittings can now be stored and maintained directly in a workgroup folder. No more need to navigate to the workgroup folder in the Finder / Explorer.

### Mix & match single and dual use hinges

interiorcad 2025 F2 allows the use of hinges for single use (door hinged to cabinet side) in a dual use context (door hinged to cabinet partition) and vice versa.

### Horizontal blind fronts

In addition to vertical blind fronts (fake door) interiorcad 2025 F2 now provides horizontally oriented blind fronts (fake drawer front).

### Fixes

- Continuous front / back stiles now split front / back stretcher correctly
- The descriptions of all parts of the Plinth 3D are correctly shortened by the file name filter of the exports
- Divisions of cabinet were always translated to absolute dimensions upon creation in the dialog (F2.1)

### Improvements / Fixes NC-Export / Cuttinglist-Export

- BiesseCIX / bSolid - In order to use the Lamello Clamex properly, it is necessary to override the original side generated by the NC macro and define a separate side in the NC macro code of the Clamex. To override the original side the strings "NAME=WFL" and "sideid" must be in the NC macro code. If this is the case, the side properties change their functionality.

### Improvements Libraries

- Lamello P-System 2024 with Drilling 3D and improved alignment for the following systems

- bSolid
- Zeta P2 handheld machine - drillings for positioning pins

- Hettich AvanTech YOU 2024 - series now with separate front fixings
- Hettich Frontstabilizer - new model

# Release Notes interiorcad 2025 F1

### Fixes

- Drillings and center punches of integrated mounting plates sometimes would not export properly
- AV list considers edge length addition
- 'Remove NC info' added to interiorcad workspaces
- Cabinet 3D - Deleting saved fitting configurations caused a crash

### Improvements / Fixes NC-Export / Cuttinglist-Export

- Custom Export

- Construction group of fittings was stile / shelf
- Search Filter for available fields
- The field thickness now outputs the overall thickness
- New field for thickness of backing material / covering
- Filter fittings by supplier(s)

- NC-Export in general

- NC Macro Code - new variable clamexcangleverticalplus180 for special cases of the Lamello Clamex, which adds 180 degrees to the clamexcangle when used on the vertical surface

- Maestro CNC - Tool configuration file (*.tlgx) was not found if only the name was entered instead of the full path
- Xilog Plus - "Parking position distance to workpiece" can now be empty

### Improvements Libraries

- Lamello P-System 2024 with Drilling 3D and improved alignment for the following systems

- F4Integrate
- Maestro CNC
- NC-Hops
- woodWOP
- Xilog Plus

- Egger - Top 60 textures from the scopes wood, plain and design
- FixChip nesting connectors for the following systems

- bSolid
- Maestro CNC

- Hinges "Inset Application" with indication of door overlay

### Upcoming service pack

interiorcad 2025 F5 scheduled for the week of May 26, 2025.

interiorcad 2025 F4 interiorcad 2025 F3 interiorcad 2025 F2 / F2.1 interiorcad 2025 F1 Upcoming service pack