# Release Notes interiorcad 2025 F7

### Improvements

- Changing the position in the dialog "Project-Details" now asks if the position assignment in the document should be removed
- Auto-Import now supports file name "Edges.txt"

### Fixes

- Feet will be visualized again in the "Settings..." dialog of Cabinet 3D. In order to improve performance, integrated fittings and Box Objects will not be visisulized neither in the dialog preview panes nor in the VW resource manager for Cabinet 3D template objects
- Integrated Cabineo fitting was not exported properly
- Some menu commands were active although there was no open Vectorworks document

### Improvements / Fixes NC-Export / Cuttinglist-Export

- Log-file "XG Export Log.txt"

- The associated archive file now has a headline again
- The log file for Corpora integration has been renamed to ‘interiorcad Corpora Integration Export Log.txt’ and is now located in the user folder

# Release Notes interiorcad 2025 F6

### Improvements

- Repairing object connections no longer renames objects by default. If objects have to be renamed, all part layouts referencing these objects will be updated
- Integrated connectors can be created via fitting configurations even if connected parts are turned off

### Fixes

- Mirrored grid drillings are properly migrated from older versions
- Canceling the assignment of fitting configurations via the Cabinet 3D's Object Info Palette no longer regenerates the Cabinet 3D object
- Bill of materials sometimes generated wrong numbers
- Assigning project details via the Cabinet 3D Object Info Palette took too long
- Updating a Cabinet 3D object with external fittings took too long for some configurations
- Performance of opening the Cabinet 3D's "Settings" dialog improved for some configurations
- Changing the name of a Cabinet 3D via the Object Info Palette took too long

### Improvements / Fixes NC-Export / Cuttinglist-Export

- Maestro CNC's XConverter now also converts XCS scripts into PGMX files for Maestro LAB

### Improvements Libraries

- New: Würth plinth adjustment feet in all versions
- Fix: Hettich Sensys hinges for thin doors – drilling depths adjusted
- Update: Wooden drawer presets expanded
- Fix: Blum Movento S – drillings at 243 mm removed

# Release Notes interiorcad 2025 F5

### Fixes

- Sometimes angled cabinets generated too many dados for a single back
- Movable Shelves - Standard length reduction was not applied to movable shelves if triggered by a change in the front design
- Cost centers could no longer be renamed or sorted
- Length of integrated wooden drawers without additional front panel was different to the length of external drawers with equivalent configuration
- If no accessories for system drawers from the current supplier are found in the database, accessories for other suppliers are shown
- Fitting configuration was flagged as inconsistent although all three hinge types were present
- Grid #(32mm*2) did not work on small parts
- Export boxobject symbol - Saving in library is now the default
- Opening the cabinet settings dialog was really slow if the cabinet contained a substantial number of parts and external routings

### Improvements / Fixes NC-Export / Cuttinglist-Export

- Custom Export

- "NC program name (with separator)" may have generated an empty list or a TypeError

- Cuttinglist-Exports

- Cuttinglist-Export AK-Soft (CH), Swiss-Soft (CH) and Triviso ERP (CH) better named
- Triviso ERP (CH) - Decimal separator permanently set to point so that the import of odd numbers always works

- NC-Exports

- F4Integrate - custom variable section, among other things, for the FixChip for surfaces as variables and for Clamex tools
- NC-Hops - variables in the "NC-Hops Variables.txt" have been added for the assignment of the dowel macro

### Improvements Libraries

- New: Nova Pro Scala now also available from supplier Würth
- New: FixChip for F4Integrate
- New: Häfele underfloor runners from the Matrix Runner UM A30/50 series
- New: Häfele system drawers from the Matrix Box Slim A series
- Update: Grass Nova Pro color Zircon for drawer heights H63, H90, H122, H186, H250
- Update: Grass Nova Pro longside rails with front support removed
- Fix: Häfele Lamello P-System for Maestro CNC - milling mode adjusted
- New: Material presets for wooden and system drawers
- Update: Grid for dowels, screws, and connectors adjusted and expanded
- Fix: Small grids starting from the center optimized

# Release Notes interiorcad 2025 F4

### Performance Box Objects

Selecting, loading and creating Box Objects was sped up substantially.

### Please note - Own Box Objects

If you have created your own box objects in your user or workgroup folder, please open and re-save these files.

### Material Description / Comment (Preview)

The field "Description" of a Custom Part 3D's material is now mirrored in the Custom Part 3D's object info palette and can be edited there.

The value of the field "Description" of a Custom Part 3D's material now remains if a material set containing no description is loaded.

The value of the field "Comment" of a Custom Part 3D's material now remains if a material set containing no comment is loaded.

### Fixes

- External grid grillings were not migrated properly from previous versions (F4.2)
- Part-based external grid drillings were not exported correctly to Part Layout or NC-Export (F4.2)
- Top/Bottom distance of external grid drilling was mixed up if placed on a Cabinet 3D's right side (F4.2)
- Grid drillings on partitions based on a fixed shelf were not exported correctly to Part Layout or NC-Export (F4.2)
- Choosing custom box objects sometimes terminated Vectorworks unexpectedly if the custom box objects were located in nested folders within the user folder (F4.2)
- Material sets were not always loaded from the workgroup folder (F4.1)
- Integrated grid drilling created a spare drilling if applied to multiple boxes with grid drilling turned off
- When saving a fitting configuration, interiorcad sometimes complained that the configuration is empty
- Fitting configuration sometimes were reported as being inconsistent
- Continuous partitions designed as mitered were not created properly if the angled part was defined as a top board
- Depending on the selection, fittings were exported inconsistently
- 2D view of Cabinet 3D did not include a laid-on back
- Symbols contained in Box Object sets were not saved in workgroup folders
- Loading a set for fixed shelves reset option to turn off grid drilling in the cox containing the fixed shelf
- Dialog to edit fitting configurations did not show source of fitting configuration file (user / workgroup folder)
- Applying a fitting configuration stored in a workgroup folder did not apply drawers
- Option to open user and workgroup folder were mixed up in Cabinet 3D "Construction" dialog pane
- Integrated grid drillings could not be based on grids stored in workgroup folder
- Overwriting an existing fitting configuration sometimes removed another configuration
- Front details text on Cabinet 3D front panels was not formatted and aligned properly
- Fixes for migrating workgroup folders from older versions
- Custom system drawers stored in workgroup folders did not show up in Drawer 3D tool's mode bar
- Fittings placed on an angled Cabinet 3D object were created outside the cabinet
- Integrated drawers configured with previous versions did not show up with the correct specification in the Cabinet 3D's settings dialog
- Drill-through / route-through drillings and contours were not created with the correct depth in integrated wooden drawers
- Partitions for angled cabinets (front view) were not created properly if the option "Automatic" was set for the creation of angled parts and the cabinet's side / board thickness were different

### Improvements / Fixes NC-Export / Cuttinglist-Export

- productionManager (HOMAG) as new Cuttinglist output format

- The export creates a ZIP file with a user-definable path and name
- The parts list configuration contains further options for customizing the output
- Technically the ZIP file contains

- an XML file with a hierarchical structure according to project item, cabinet and custom part, each with all associated production details
- the simultaneously or previously created NC programs stored in subfolders of the same hierarchy

- In productionManager, the ZIP file can be opened using the command "Import new job"

- NC-Export in general

- WorkpieceComments extended: SupplierID, Length, Width, Thickness, BoardThickness, Covering1Thickness, Covering2Thickness, SetName, HasCovering, HasSizing

### Improvements Libraries

- New: Häfele screws - Washer head screws for back panels
- Update: Häfele screws - Sales info updated
- Update: Custom Part 3D materials now with empty description
- Update: Lamello P-System Connectors for Maestro CNC Schreinertraum
- Fix: Hettich Sensys hinge for inset applications now has correct secondary drillings

# Release Notes interiorcad 2025 F3

### Fixes Sets

- Use the new searchable pulldown menu to disclose and find sets located in the vectorworks defaults folder, user folder or workgroup folder easily
- Navigate to the current user or workgroup folder right from within each set pulldown menu
- New searchable pulldown menu to access Cabinet 3D material sets in settings dialog and, for all sets, in Cabinet 3D's object info palette

### Fixes Drawers

- Custom suppliers were ignored for integrated sliders
- Occasionally, sets and fitting configurations couldn't be assigned
- Integrated wooden drawers / sliders can now be inset from the front of the Cabinet 3D

### Other Fixes

- Profiles can now be placed on custom parts with non-standard oriented paths using either interiorcad's profile tool or Vectorworks' symbol insertion tool
- Option "Interrupt grid drilling" is available if no grid drilling is assigned tothe Cabinet 3D object yet (e.g. for using a fitting configuration)
- Dado for back was too short for angled Cabinet 3D
- Horizontal / Vertical blind fronts have separate 2D/3D representation now
- Using integrated drawers sometimes added an additional slider right at the cabinet's insertion point
- Changing height of Cabinet 3D multiple times sometimes caused Vectorworks to quit unexpectedly
- Grid drillings on angled cabinets (viewed from the right) were not created properly after transforming the cabinet
- Continuous partitions dividing a slanted top board were not created properly
- Inset dados were not created properly for slanted parts of an angled cabinet

### Improvements / Fixes NC-Export / Cuttinglist-Export

- Custom Export

- The material properties -> Part (item number) -> supplier id and description were not transferred

- Cuttinglist-Export in general

- Box objects of different lengths are not cumulated

- Maestro Ottimo Cut - Incorrect conversion of the fixed date fixed
- NC-Export in general

- Clamex machine configurations and error messages improved
- The new Clamex fittings may have generated a TypeError when using {clamexcangle}.

### Improvements Libraries

- New Special Connectors: FESTOOL Domino corner and worktop connectors (plus extra FESTOOL grids)
- New System Drawers: Häfele Matrix Box P Plus as a set available in heights of 60 mm / 115 mm / 170 mm (custom heights in combination with Longside Rails)
- New Sliders for Wooden Drawers: Grass Dynaneo
- New Hinges and Mounting Plates: Grass MB object hinges
- Fix: Hettich ArciTech Drawer Boxes with Longside Rails

# Release Notes interiorcad 2025 F2 / F2.1

### Saved sets & fittings in workgroup folders

Saved sets & fittings can now be stored and maintained directly in a workgroup folder. No more need to navigate to the workgroup folder in the Finder / Explorer.

### Mix & match single and dual use hinges

interiorcad 2025 F2 allows the use of hinges for single use (door hinged to cabinet side) in a dual use context (door hinged to cabinet partition) and vice versa.

### Horizontal blind fronts

In addition to vertical blind fronts (fake door) interiorcad 2025 F2 now provides horizontally oriented blind fronts (fake drawer front).

### Fixes

- Continuous front / back stiles now split front / back stretcher correctly
- The descriptions of all parts of the Plinth 3D are correctly shortened by the file name filter of the exports
- Divisions of cabinet were always translated to absolute dimensions upon creation in the dialog (F2.1)

### Improvements / Fixes NC-Export / Cuttinglist-Export

- BiesseCIX / bSolid - In order to use the Lamello Clamex properly, it is necessary to override the original side generated by the NC macro and define a separate side in the NC macro code of the Clamex. To override the original side the strings "NAME=WFL" and "sideid" must be in the NC macro code. If this is the case, the side properties change their functionality.

### Improvements Libraries

- Lamello P-System 2024 with Drilling 3D and improved alignment for the following systems

- bSolid
- Zeta P2 handheld machine - drillings for positioning pins

- Hettich AvanTech YOU 2024 - series now with separate front fixings
- Hettich Frontstabilizer - new model

# Release Notes interiorcad 2025 F1

### Fixes

- Drillings and center punches of integrated mounting plates sometimes would not export properly
- AV list considers edge length addition
- 'Remove NC info' added to interiorcad workspaces
- Cabinet 3D - Deleting saved fitting configurations caused a crash

### Improvements / Fixes NC-Export / Cuttinglist-Export

- Custom Export

- Construction group of fittings was stile / shelf
- Search Filter for available fields
- The field thickness now outputs the overall thickness
- New field for thickness of backing material / covering
- Filter fittings by supplier(s)

- NC-Export in general

- NC Macro Code - new variable clamexcangleverticalplus180 for special cases of the Lamello Clamex, which adds 180 degrees to the clamexcangle when used on the vertical surface

- Maestro CNC - Tool configuration file (*.tlgx) was not found if only the name was entered instead of the full path
- Xilog Plus - "Parking position distance to workpiece" can now be empty

### Improvements Libraries

- Lamello P-System 2024 with Drilling 3D and improved alignment for the following systems

- F4Integrate
- Maestro CNC
- NC-Hops
- woodWOP
- Xilog Plus

- Egger - Top 60 textures from the scopes wood, plain and design
- FixChip nesting connectors for the following systems

- bSolid
- Maestro CNC

- Hinges "Inset Application" with indication of door overlay

### Upcoming service pack

interiorcad 2025 F8 is not yet planned.

interiorcad 2025 F7 interiorcad 2025 F6 interiorcad 2025 F5 interiorcad 2025 F4 interiorcad 2025 F3 interiorcad 2025 F2 / F2.1 interiorcad 2025 F1 Upcoming service pack