# Release Notes interiorcad 2026 F4

### Improvements

- Box objects can now be transferred via "Copy / Paste" in Cabinet 3D's preview
- Non-rectangular Cabinets can now be defined by knee wall height plus angle

### Fixes

- Dado insets of integrated wooden drawers were not exported properly
- Newly created door of a non-rectangular cabinet was not visualized properly in preview
- Moving an integrated wooden drawer along the y-axis was not updating the drawer length accordingly
- Profiles applied to horizontal blind fronts were not oriented correctly
- Tool icons in workspaces appeared out of focus
- Changing the name of Custom Part 3D via Object info palette took a long time, especially in complex documents
- Option "With Boxobjects" was not functional when saving a set
- Integrated hinges did not follow the change of hinged side
- Some box objects eligible for a front box were not shown in the pull-down menu
- Mirrored Plinth 3D created wrong recesses for parts
- Grid drillings were not loaded properly from fitting configurations
- Images in dialog "Cabinet settings" are properly scaled and positioned if screen zoom factor is set to values not equal to 100% (Windows)

### Improvements / Fixes NC-Export / Cuttinglist-Export

- Update of the 2WOP scope of performance and the output formats F4®Integrate, GANNOMAT Editor ASCII, Maestro CNC/Lab and NC-Hops (4-8)
- Custom Export
  - Default field delimiter for new Custom Exports set to semicolon
- NC-Export in general
  - The "Clear out Contour 3D" option is not applied to open contours. Open contours are always output as regular contours during export.
  - woodWOP - Corrected "Maximal length in x direction of sections for rabbets and milled dados"

### Improvements Libraries

- New
  - Door and window presets for the "Simple Wall" object
- Update
  - interiorcad.sta updated with new classes and class filters
  - interiorcad.sta updated with activated databases for the use of worksheets and data stamps

# Release Notes interiorcad 2026 F3

### Improvements

- Improved performance when selecting box objects at point of use
- Substantially improved options to design backs for angled cabinets (view from right)
- Show relevant dialog pane only when using the object info palette buttons (Preview)
- Part layout - hide / show parts of plinth frame
- New menu command "Convert to simple walls..." (interiorcad Starter)
- "Plinth 3D" - Mode "Create plinth from selected objects" can now be applied to grouped Cabinet 3D objects

### Fixes

- Custom dimensions of dialogs to choose materials from database were not stored properly
- Sometimes, integrated hinges could not be aligned with grid drillings
- Integrated drawer depth was not properly set
- Material of an integrated drawer could not be changed
- Edge configuration of Plinth 3D was not stared properly
- Blind front 2D/3D settings were not stored in sets
- Choosing board materials sometimes showed wrong board thickness
- In Cabinet 3D's settings dialog, clicking on a partition or left / right side of cabinet sometimes opened up materials settings for selected part
- Thickness of solid materials could not be edited in Custom Part 3D's object info palette

### Improvements / Fixes NC-Export / Cuttinglist-Export

- Cuttinglist-Export in general
  - Materials of different thicknesses
    - The maximum thickness is used in the cumulative material list
    - There is no accumulation in the parts list, so that different thicknesses - e.g. for planed solid wood - are shown separately
- NC-Export in general
  - DXF attribute "elevation" as an alternative to "thickness" for Z values explicitly for contour lines (LWPOLYLINE) - preferred by Vectric VCarve
  - Wood Flash - Control of the formatting macro added

### Improvements Libraries

- New
  - Grass Vionaro V8 available as sets from Würth
  - Grass Vionaro V13 available as sets from Würth
  - Door and window presets for the “Simple Wall” object
  - Automatic data stamp for Cabinet 3D, Plinth 3D, and Custom Part 3D
- Update
  - Häfele Matrix Box P Plus longside rails with glass insert
  - Lamello Cabineo flush-mounted now available as a drilling–milling combination
  - Häfele Blum Movento and Tandem with new order numbers
- Fix
  - Added missing sliders for Häfele Legrabox
  - Added missing Zeta drillings for the Häfele Lamello P-System

# Release Notes interiorcad 2026 F2

Known problems in interiorcad 2026 F2

- On macOS, interiorcad's fitting tools don't use the X-Ray Select mode and turn on Wireframe mode instead.

### Improved material type "solid"

Materials of type "solid" can now be assigned edges and coverings.

### interiorcad Viewer

The Vectorworks Viewer can be enhanced with interiorcad functionality in order to allow the inspection of complex interiorcad object settings e.g. Custom Part, Plinth, Drawer or Cabinet.

### Box objects on point of use

Box objects can now be configured right next to the integrated fittings of the cabinet.

### Plinth Cabinet / Plinth 3D

- An addition plinth frame can be defined
- The configuration of plinth part dimensions and location was improved
- Plinth 3D now features material sets (for both plinth and plinth frame)

### Improvements / Fixes NC-Export / Cuttinglist-Export

#### Custom Export

- Output format names are now identical to their original counterparts plus (Custom)
- Adding an empty replacement table is now prevented

#### Cutting list exports

- productionManager
  - Hierarchy level reduced to Position_Cabinet - Parts
  - Relative path for NC program names adapted for folder structure on machines
  - Article number and description swapped
  - Article group added
  - The fields article description, group, and number can be adjusted in the production settings

#### NC-Exports

- General
  - New placeholder for path {PositionNumber_CabinetName} matching the productionManagers hierarchy
- Wood Flash - Feed rate added for the first segment
- woodWOP - Differentiated labels for sizing, vertical routing, vertical dado, rabbet, horizontal and horizontal dado
- Xilog Plus - Sizing with A0_SFORM macro including miter saw and settings

### Improvements Libraries

- New
  - FixChip for woodWOP
  - Construction and material set for the Plinth 3D object
- Update
  - Removed old versions of P-System connectors
  - Cleaned up Blum Tandem series - removed several symbols that are no longer available
  - Added Grass Vionaro H121 NL650
  - Häfele Axilo 78 mounting plate with new geometry and order number
- Fix
  - Corrected numbering errors in some symbol names of the Grass Dynapro series

# Release Notes interiorcad 2026 F1

The feature set of interiorcad 2026 F1 is equivalent to interiorcad 2025 F7 (with the only difference being based on Vectorworks 2026, of course). New interiorcad features will be released with interiorcad 2026 F2 and subsequent updates.

### Upcoming service pack

interiorcad 2026 F5 scheduled for the week of May 22, 2026.

interiorcad 2026 F4 interiorcad 2026 F3 interiorcad 2026 F2 interiorcad 2026 F1 Upcoming service pack